**The existing technology and the application of digital artificial intelligent in the wastewater treatment area: A review paper**

**Sri Martini1, Kiagus Ahmad Roni**

*Faculty of Engineering, Chemical Engineering Department, Universitas Muhammadiyah Palembang, 13 Ulu Palembang, Indonesia.,*

*email:* [*srimartini79@gmail.com*](mailto:srimartini79@gmail.com)and [*kiagusaroni@gmail.com*](mailto:kiagusaroni@gmail.com)

*1Corresponding author*

**Abstract.** Wastewater treatment using various existing technologies including advanced oxidation processes, adsorption, and membrane separation for various pollutants removal from industrial and municipal wastewater streams is an essential aspect of reaching environmental sustainability, keeping human well-being and healthy economic growth. However, there are some challenging aspects along with the wastewater treatment process affecting pollutant removal efficiency and other resources. This condition will lead to various uncertainty in the wastewater treatment system related to the fluctuations in the quality of treated water and wastewater, operation costs, and the environmental risk. Artificial intelligence then can be such a reliable solution tool to predict and minimize those complications and optimize the process and parameters implemented in the wastewater treatment system.

**Keywords:** Wastewater treatment, adsorption, membrane filtration, artificial intelligent, circular economy

1. **Introduction**

These days the terms of circular economy, waste management, and digital artificial intelligent have drawn increasing attention globally from many relevant stakeholders, including government, academics, and industrial parties. This phenomenon is derived from the need of practical ways to solve some issues related to the growing volume of industrial and municipal wastewaters that can be a challenge for reaching relevant goals associated with the economic growth and environmental sustainability. Thus, it is necessary to manage waste with several strategies, including by reducing material consumption and replacing conventional management with more modern ones.

This strategic treatment is primarily intended for industry and agriculture because of the linear economic relationship between the strategy and the existing problems [[1](#_ENREF_1), [2](#_ENREF_2)]. Polluted water and wastewater streams threat human health, other living creatures, and environmental sustainability as a whole as they could contain oil and grease, heavy metals, dyes, phenol, or other harmful contaminant particles. These wastewaters are commonly released into the environment from various growing industrial sectors such as petroleum refinery, textiles, pulp and paper, tanneries, plastics, mining, brass and bronze manufacturing, steel production, electroplating, pharmaceuticals, galvanizing, pigments, insecticides, cosmetics, battery manufacturing, paints, and pigments [[3](#_ENREF_3), [4](#_ENREF_4)].

The increasing number of world population has resulted in the growing demand in many human needs, especially food and energy. This has caused more unwanted by-products and agricultural residues given a more significant challenge to the development of the circular economy concept. Therefore, digital applications' involvement in predicting and optimizing the process of treating industrial and municipal wastewaters to enable the treated water reusable for further productive usage is inevitable [[5](#_ENREF_5)].

Furthermore, artificial intelligence has been used widely in many engineering disciplines as it offers reliable solutions to solve practical problems, including wastewater treatment and machine fault analysis [[6](#_ENREF_6), [7](#_ENREF_7)]. Concerning various existing technologies for water and wastewater treatment such as the adsorption process, membrane filtration, and advanced oxidation processes [[8](#_ENREF_8), [9](#_ENREF_9)], the application of artificial intelligent or machine learning system is reliable and resourceful. Therefore, the main aims of this review paper are to further focus on giving information related to the available methods for water and wastewater treatment and relevant literature regarding the practical application of artificial intelligence as a digital transformation tool in wastewater treatment area, so the reusable components that enable less or zero waste to support circular economy society can be manifested.

**2. Existing technologies for water and wastewater treatment**

*2.1 Adsorption process*

Adsorption could be defined as atoms or ions accumulation process from gas, liquid, or concrete to adsorbent pores or surface forming a typical layer of the adsorbate. Various pollutant particles, including oil and grease, dyes, metal ions, dissolved solid or other organic and non-organic compounds can be part of the adsorbate typical layer [[10](#_ENREF_10), [11](#_ENREF_11)]. Activated carbon, biochar, and chemically modified adsorbent are well-known adsorbent types used in various industrial wastewater treatment plants. Those adsorbent materials could be derived from synthetic, organic, and non-organic materials. Furthermore, to maintain environmental sustainability, some efforts are made to use natural materials, namely plant-based adsorbents such as eucalyptus bark, banana peels, barley straw, watermelon peels, orange peels, and other organic materials for the removal of targeted pollutants [10-19].

*2.2 Membrane filtration*

Membrane filtration is a superior technology to remove various pollutants resulting in treated water with a high purity level, so it could be reused for different purposes, such as processing water, irrigation, and even drinking water [[12](#_ENREF_12)]. Based on the particles' size and character, membranes can be categorized into microfiltration, ultrafiltration, nanofiltration, and reverse osmosis. Compared to other treatment methods, the membrane's filtration usage has shown outstanding work for their high efficiency, including oil, dyes, and massive metals depletion [[13-15](#_ENREF_13)]. However, membrane materials are vulnerable to the fouling phenomenon occurring by the time of operation. Fouling is caused by deposited pollutant particles on membrane pores and surface reducing permeate flux. In order to lower fouling rate, several approaches such as periodic washing, pre-treatment stage, and other optimization processes are needed [[15](#_ENREF_15), [16](#_ENREF_16)].

* 1. *Advanced oxidation*

Advanced oxidation processes (AOPs) are characterized by radical hydroxyl production responsible for targeted organic and non-organic pollutants removal. The pollutants can be transformed into water, carbon dioxide, and other harmless products. There are various ways of performing AOPs, including Fenton (H2O2/Fe2+), Fenton-like (H2O2/Fe3+), electron beam irradiation, sonolysis, electrochemical oxidation, photo-assisted Fenton (H2O2/Fe2+/Fe3+/UV), and photo-catalytic reaction (TiO2/O2, O3/ H2O2, O3/UV, H2O2/UV) [[17-20](#_ENREF_17)]. Literature has shown the efficacy of these methods to put targeted pollutants at bay [[21](#_ENREF_21), [22](#_ENREF_22)]. Nevertheless, several shortfalls of these methods need to be concerned, such as costly chemical usage and its after-use impacts, sludge generation, and by-product formation.

*2.4. Coagulation and flocculation*

Coagulation and flocculation are prominent methods used for treating contaminated water, primarily in the initial step to remove dissolved and suspended solid particles and other organic and non-organic pollutants through the application of flocculants and coagulants media such as aluminium and ferric chloride [[12](#_ENREF_12)]. This process involves some influential parameters such as initial targeted pollutants concentration, coagulants and flocculants agent dosage, and pH of the solution. This process also consists of several principles like destabilization, entrapment, and aggregation or colloids binding stages to form larger and heavier flocks of pollutants particles, so it would be easily removed by subsequent settling and filtration stages. However, some concern could be directed to avoid disadvantageous sides of using this method including costly coagulant and flocullant reagent, excessively abundant sludge production for continuous and large treatment plant, and toxic sludge disposal in the environment that also need further solution [[23](#_ENREF_23)].

*3.3. Biological process*

Various microorganisms types like abundantly available in nature including fungi, bacteria, yeast, and algal biomass are involved in the degradation pollutant process in contaminated solution during biological method. Even though it has some drawbacks including longer reaction time and wider treatment treatment plant area, some biological approaches including trickling filter and activated sludge could be simple and more environmentally friendly as well as more cost-effective than other treatment modes. In terms of the need of oxygen, biological agents can be devided into aerobic and anaerobic types, however, combined aerobic–anaerobic microorganisms were implemented in certain condition to get better results [[24-26](#_ENREF_24)].

* 1. *Integrated method*

Considering no wastewater treatment techniques could be used individually to obtain both effective and efficient points with the highest standard of treated water, several existing technology in this area including membrane filtration, adsorption, coagulation, flocculation, and chemical oxidation which have their own shortcomings should be integrated well. Some studies have proved that this integration could benefit the process and enable us to reach better quality of wastewater with better machine and other treatment media condition.

The hybrid of adsorption using hybrid powdered activated carbon and membrane filtration, for example, has been investigated and reported to be reliable and satisfactory by some previous studies [[27](#_ENREF_27), [28](#_ENREF_28)]. This is because powdered activated carbon could better feed circulation even in low concentration. It can create shear stress on the membrane surface. This effect could reduce cake layer thickness leading to the high permeation flux and pollutant removal efficiency reducing fouling rate. Other integrated treatment methods can be derived from the same field such as using dual membrane processes. Two different types of membrane named ultrafiltration and reverse osmosis membrane have been investigated for treating oily wastewater containing high initial oil and COD concentration. The study then reported that this dual membrane system could yield about only 7 % of permeate flux decline with free suspended solid, high TOC and cations removal efficiency in the treated wastewater [[29](#_ENREF_29)]. However, the implementation of dual membrane system could be restricted to the high cost for constructing and maintaining the system. The development of integrated system consisting of two or more treatment methods has some advantages that can be related to higher quality of treated water and wastewater as well as providing safer condition for expensive and complex machinery used in the plants such as membrane filtration plant. A study applying advanced oxidation on wastewater as a pre-treatment stage before entering polymeric ultrafiltration membrane reported a massive reduction of fouling rate leading to lesser washing cycles and longer membrane lifespan [[9](#_ENREF_9)].



Fig. 1 Integrated wastewater treatment technology involving advanced oxidation processes and membrane filtration.

1. **Artificial intelligent applied in wastewater treatment technology**

In the last decade, research has focused on digital application or machine learning to improve pollutants removal and benefit both economic and efficient energy levels. This artificial intelligent implementation has been implemented into various aspects such as wastewater treatment, waste management, and resource extraction and reuse [[30](#_ENREF_30)]. In accordance with its specific usage, digital machine learning has been applied in wastewater treatment field related to prediction and optimization purposes. This efforts have been developed to get more reliable real calculations that could give some benefits in term of the use of chemicals in adsorption or advanced oxidation methods or the costly replacement of membrane materials due to fouling phenomena.

Most artificial intelligent techniques were modeled using experimental data to simulate, predict, confirm, and optimize targeted pollutants removal in wastewater treatment processes. In general, the experimental data set is divided into three groups, namely training data, validation data, and testing data. Or it can also be divided into two groups, namely training data and testing data, with training data used as an initial development model. Meanwhile, the validation data is used to optimize the modeling so that the test data function can be applied in the whole data to predict the final model. In other words, model performance results from the test involve the comparison of the experimental data in the predicted data to obtain better correlation coefficient (R2), performance efficiency, accuracy, and integral of the squared error [[30](#_ENREF_30), [31](#_ENREF_31)].

In adsorption process, for example, a study about the adsorption of heavy metal named arsenic from aqueous solution using plant-based adsorbent made from Opuntia ficus indica biomass that was previously activated by pyrolysis and ZnCl2 used its experimental data to further study kinetic and isotherm pattern [[32](#_ENREF_32)]. In order to set a new isotherm and kinetic equations, they also developed a modelling using the hybridization of the traditional adsorption equations with an artificial neural network. The artificial neural network then was used to improve the performance of the initial conventional kinetic and isotherm equations for making the simulation of arsenic removal at varying pH and temperature. Furthermore, the performance of models applied was examined using arsenic adsorption experimental data resulting in the outperformed model representing kinetic and isotherm adsorption equations for the better calculations of process design. Several prominent digital modeling stated in literature can be seen in Table 1.

**Table 1.** Typical artificial intelligent applied as a machine learning tool in the wastewater treatment system

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Artificial intelligent name | Treatment technology | Function | Ref. |
| 1 | Artificial neural network | Membrane filtration | To predict transmembrane pressure and fouling occurrence | [[33](#_ENREF_33)] |
| 2 | Fuzzy logic | Adsorption | To predict Pb(II) removal efficiency using activated carbon nanocomposite | [[34](#_ENREF_34)] |
| 3 | Genetic algorithm | Adsorption | To produce better adsorption bed and adsorbent porosity | [[35](#_ENREF_35)] |
| 4 | Data mining | Activated sludge | To optimize the activated sludge process and minimize energy | [[36](#_ENREF_36)] |
| 5 | Response surface methodology | Coagulation and flocculation | To optimize the independent parameters for better pollutant removal | [[37](#_ENREF_37)] |
| 6 | Bayesian network | Modified sequencing batch reactor | To model and optimize wastewater treatment plant | [[38](#_ENREF_38)] |
| 7 | Support vector machine | Adsorption | To predict drug reduction effect and improve pollutant removal | [[39](#_ENREF_39)] |
| 8 | Linear regression | Membrane filtration | To predict the permeate rate and fouling mechanism | [[16](#_ENREF_16)] |

In terms of treating wastewater using membrane method, this digital machine learnings including artificial neural network could also be a competitive alternative for dynamic cross-flow ultrafiltration modelling as its application for predicting flux decline occurred during filtration process is reliable [[40](#_ENREF_40)]. The cross-flow ceramic ultrafiltration membranes has been modelled using artificial neural networks for assessing the multilayer perceptron. For this reason, several crucial operating parameters such as transmembrane pressure, cross-flow velocity, and filtration time as well as dynamic fouling were used as input data to predict the behaviour of permeate flux. The authors did several pre-treatments of the experimental data and the optimal selection of the parameters of the neural networks to improve the fitting accuracy which was then compared to well-known Hermia pore blocking models. Considering the computational speed, high accuracy and the ease of the artificial neural networks. They concluded that fitting accuracy of artificial neural network model is comparable to that of Hermia’s models which was adapted to the cross-flow ultrafiltration. Specifically, it was similar to those previously obtained for Hermia’s intermediate blocking model in high trans membrane pressure condition.

Other artificial intelligent that could be utilized to benefitting wastewater treatment area is fuzzy logic application. A study used this digital type for predicting and controlling wastewater to be recycled, so it could meet standardised quality value of water and wastewater for further usage including for agricultural and industrial purposes [[41](#_ENREF_41)]. The surrogation of wastewater treatment plant could avoid simulating complex physical, chemical, and biological treatment processes that prominently faced by conventional methods. Each fuzzy logic model enable to predict water quality parameters by measuring influent water quality parameters such as biochemical oxygen demand (BOD), chemical oxygen demand (COD), pH, temperature, and total suspended solid. A supervised committee fuzzy logic (SCFL) model consisting of three fuzzy models named Takagi-Sugeno, Mamdani, and Larsen can be applied as a predictive ensemble model. This model combined with an [artificial neural network](https://www-sciencedirect-com.dbgw.lis.curtin.edu.au/topics/earth-and-planetary-sciences/artificial-neural-network) to include the forecasted water quality resulted from individual fuzzy logic models. To conclude, the individual fuzzy logic models have had a mean absolute percentage error (MAPE) for BOD, COD and TSS in the testing stage ranging from 10 to 13%. While the SCFL model could reduce MAPE value to 4% in the testing step.

1. **Summary**

In this review article, some existing standard technologies implemented for the wastewater treatment area are explained. Because industrialization and the speed of population growth have increased from contaminated water sources that threaten the health of the population and damage the environment, an environmentally friendly waste treatment technology is needed with the least possible waste output. Another essential alternative is to reduce energy consumption, which has a very immediate impact on the environment and human life. Following that notion, optimization algorithms as digitally intelligent techniques will help optimize the significant parameters related to some aspects of wastewater treatment plants, such as predicting and reducing membrane fouling rate and optimizing adsorption capacity adsorbent in the adsorption process. To conclude, machine learning in a wastewater treatment study is a better option for gaining a circular economy society with better environmental conditions.

1. **Reference**

[1] P. Kerdlap, J.S.C. Low, S. Ramakrishna, *Zero waste manufacturing: A framework and review of technology, research, and implementation barriers for enabling a circular economy transition in Singapore*, Resources, Conservation and Recycling, 151 (2019) 104438.

[2] C.-Y. Young, S.-P. Ni, K.-S. Fan, *Working towards a zero waste environment in Taiwan*, Waste Management & Research, 28 (2010) 236-244.

[3] S. Martini, *Development of an Efficient Integrated System for Industrial Oily Wastewater Treatment*, in, Curtin University, 2016.

[4] R. Chakraborty, A. Asthana, A.K. Singh, B. Jain, A.B.H. Susan, *Adsorption of heavy metal ions by various low-cost adsorbents: a review, International Journal of Environmental Analytical Chemistry*, (2020) 1-38.

[5] A.M. Ghaedi, A. Vafaei, *Applications of artificial neural networks for adsorption removal of dyes from aqueous solution: A review*, Advances in Colloid and Interface Science, 245 (2017) 20-39.

[6] S. Al Aani, T. Bonny, S.W. Hasan, N. Hilal, *Can machine language and artificial intelligence revolutionize process automation for water treatment and desalination?*, Desalination, 458 (2019) 84-96.

[7] X.F. St-Onge, J. Cameron, S. Saleh, E.J. Scheme, *A symmetrical component feature extraction method for fault detection in induction machines*, IEEE Transactions on Industrial Electronics, 66 (2018) 7281-7289.

[8] S.S. Beulah, K. Muthukumaran, *Methodologies of Removal of Dyes from Wastewater: A Review*, International Research Journal of Pure and Applied Chemistry, (2020) 68-78.

[9] S. Martini, H.M. Ang, *Hybrid TiO2/UV/PVDF ultrafiltration membrane for raw canola oil wastewater treatment*, Desalination and water treatment, 148 (2019) 51-59.

[10] S. Afroze, T.K. Sen, M. Ang, H. Nishioka, *Adsorption of methylene blue dye from aqueous solution by novel biomass Eucalyptus sheathiana bark: equilibrium, kinetics, thermodynamics and mechanism*, Desalination and Water Treatment, (2015) 1-21.

[11] S. Martini, S. Afroze, K.A. Roni, *Modified eucalyptus bark as a sorbent for simultaneous removal of COD, oil, and Cr (III) from industrial wastewater*, Alexandria Engineering Journal, (2020).

[12] N.P. Cheremisinoff, *Handbook of water and wastewater treatment technologies*, Butterworth-Heinemann, 2001.

[13] C. Yang, W. Xu, Y. Nan, Y. Wang, Y. Hu, C. Gao, X. Chen, *Fabrication and characterization of a high performance polyimide ultrafiltration membrane for dye removal*, Journal of Colloid and Interface Science, 562 (2020) 589-597.

[14] X. Liu, B. Jiang, X. Yin, H. Ma, B.S. Hsiao, *Highly permeable nanofibrous composite microfiltration membranes for removal of nanoparticles and heavy metal ions*, Separation and Purification Technology, 233 (2020) 115976.

[15] S. Martini, *Pengolahan limbah cair minyak kanola menggunakan kombinasi adsorpsi dan membran ultrafiltrasi polimer*, Kinetika, Kinetika, 10 (2019) 36-41.

[16] S. Martini, H.M. Ang, H. Znad, *Integrated ultrafiltration membrane unit for efficient petroleum refinery effluent treatment*, Clean Soil Air Water, 45 (2017) 1-9.

[17] R. Andreozzi, V. Caprio, A. Insola, R. Marotta, *Advanced oxidation processes (AOP) for water purification and recovery*, Catalysis Today, 53 (1999) 51-59.

[18] J.M. Ochando-Pulido, M.D. Victor-Ortega, G. Hodaifa, A. Martinez-Ferez, P*hysicochemical analysis and adequation of olive oil mill wastewater after advanced oxidation process for reclamation by pressure-driven membrane technology*, Science of The Total Environment, 503–504 (2015) 113-121.

[19] J.A. Garrido-Cardenas, B. Esteban-García, A. Agüera, J.A. Sánchez-Pérez, F. Manzano-Agugliaro, *Wastewater treatment by advanced oxidation process and their worldwide research trends*, International Journal of Environmental Research and Public Health, 17 (2020) 170.

[20] S. Martini, H.T. Znad, H.M. Ang, *Photo-assisted fenton process for the treatment of canola oil effluent,* in: Chemeca 2014: Processing excellence; Powering our future, Engineers Australia, Barton, ACT, 2014, pp. [1519]-[1533].

[21] M. Tariq, M. Muhammad, J. Khan, A. Raziq, M.K. Uddin, A. Niaz, S.S. Ahmed, A. Rahim, *Removal of Rhodamine B dye from aqueous solutions using photo-Fenton processes and novel Ni-Cu@ MWCNTs photocatalyst*, Journal of Molecular Liquids, (2020) 113399.

[22] A. Jamil, T.H. Bokhari, T. Javed, R. Mustafa, M. Sajid, S. Noreen, M. Zuber, A. Nazir, M. Iqbal, M.I. Jilani, *Photocatalytic degradation of disperse dye Violet-26 using TiO2 and ZnO nanomaterials and process variable optimization*, Journal of Materials Research and Technology, 9 (2020) 1119-1128.

[23] T.A. Kurniawan, G.Y. Chan, W.-H. Lo, S. Babel, P*hysico–chemical treatment techniques for wastewater laden with heavy metals*, Chemical engineering journal, 118 (2006) 83-98.

[24] Y.L. Pang, A.Z. Abdullah, *Current status of textile industry wastewater management and research progress in Malaysia: a review*, Clean–Soil, Air, Water, 41 (2013) 751-764.

[25] S. Mishra, A. Maiti, *Biological Methodologies for Treatment of Textile Wastewater, in: Environmental Processes and Management*, Springer, 2020, pp. 77-107.

[26] M. Gómez-Ramírez, S.A. Tenorio-Sánchez, *Treatment of Solid Waste Containing Metals by Biological Methods, in: Natural Resources Management and Biological Sciences*, IntechOpen, 2020.

[27] M.V. Sarfaraz, E. Ahmadpour, A. Salahi, F. Rekabdar, B. Mirza, *Experimental investigation and modeling hybrid nano-porous membrane process for industrial oily wastewater treatment,* Chemical Engineering Research and Design, 90 (2012) 1642-1651.

[28] T. Mohammadi, A. Esmaeelifar, *Wastewater treatment of a vegetable oil factory by a hybrid ultrafiltration-activated carbon process*, Journal of Membrane Science, 254 (2005) 129-137.

[29] M. Tomaszewska, A. Orecki, K. Karakulski, *Treatment of bilge water using a combination of ultrafiltration and reverse osmosis*, Desalination, 185 (2005) 203-212.

[30] L. Zhao, T. Dai, Z. Qiao, P. Sun, J. Hao, Y. Yang, A*pplication of artificial intelligence to wastewater treatment: A bibliometric analysis and systematic review of technology, economy, management, and wastewater reuse*, Process Safety and Environmental Protection, 133 (2020) 169-182.

[31] S.K. Bhagat, T.M. Tung, Z.M. Yaseen, *Development of artificial intelligence for modeling wastewater heavy metal removal: State of the art, application assessment and possible future research,* Journal of Cleaner Production, 250 (2020) 119473.

[32] J. Rodríguez-Romero, D. Mendoza-Castillo, H. Reynel-Ávila, D. de Haro-Del Rio, L. González-Rodríguez, A. Bonilla-Petriciolet, C. Duran-Valle, K. Camacho-Aguilar, *Preparation of a new adsorbent for the removal of arsenic and its simulation with artificial neural network-based adsorption models*, Journal of Environmental Chemical Engineering, (2020) 103928.

[33] F. Schmitt, R. Banu, I.-T. Yeom, K.-U. Do, *Development of artificial neural networks to predict membrane fouling in an anoxic-aerobic membrane bioreactor treating domestic wastewater*, Biochemical Engineering Journal, 133 (2018) 47-58.

[34] H. Javadian, M. Ghasemi, M. Ruiz, A.M. Sastre, S.M.H. Asl, M. Masomi, *Fuzzy logic modeling of Pb (II) sorption onto mesoporous NiO/ZnCl2-Rosa Canina-L seeds activated carbon nanocomposite prepared by ultrasound-assisted co-precipitation technique*, Ultrasonics Sonochemistry, 40 (2018) 748-762.

[35] S. Zhang, Z. Ge, Y. Lai, *Application of Genetic Algorithm in Optimizing a Chemical Adsorption Bed with Cacl2/expanded Graphite Adsorbent*, Procedia Engineering, 205 (2017) 1828-1834.

[36] A. Kusiak, X. Wei, *Optimization of the activated sludge process*, Journal of Energy Engineering, 139 (2013) 12-17.

[37] B. Singh, P. Kumar, P*re-treatment of petroleum refinery wastewater by coagulation and flocculation using mixed coagulant: Optimization of process parameters using response surface methodology (RSM),* Journal of Water Process Engineering, 36 (2020) 101317.

[38] D. Li, H.Z. Yang, X.F. Liang, *Prediction analysis of a wastewater treatment system using a Bayesian network*, Environmental Modelling & Software, 40 (2013) 140-150.

[39] Q.-f. Di, S. Hua, W.-p. Ding, W. Gong, Y.-c. Cheng, Y. Feng, *Application of support vector machine in drag reduction effect prediction of nano-particles adsorption method on oil reservoir's micro-channels*, Journal of Hydrodynamics, Ser. B, 27 (2015) 99-104.

[40] M.-J. Corbatón-Báguena, M.-C. Vincent-Vela, J.-M. Gozálvez-Zafrilla, S. Álvarez-Blanco, J. Lora-García, D. Catalán-Martínez, *Comparison between artificial neural networks and Hermia’s models to assess ultrafiltration performance*, Separation and Purification Technology, 170 (2016) 434-444.

[41] A.A. Nadiri, S. Shokri, F.T.C. Tsai, A. Asghari Moghaddam, P*rediction of effluent quality parameters of a wastewater treatment plant using a supervised committee fuzzy logic model*, Journal of Cleaner Production, 180 (2018) 539-549.